

**Master Your Terrain**

# (307) – 775 – 9565

[**www.tntcustoms.com**](http://www.tntcustoms.com/)

**Extreme Duty Rocker Protection Jeep CJ/VJ Wrangler**

**Installation Instructions**

Congratulations for purchasing TNT, Inc. extreme duty rocker panel protection for your Jeep Wrangler. Begin by unpacking your kit and comparing the contents to the appendi x A. Please observe proper shop safety procedures when performing this install . Use proper eye and. hearing prntection as required and use safe jack stands/supports, placed a ppropriately for:' s'upporting the vehicle while you work on it if needed.

We strongly suggest fitting the rocker guards to the vehicle a nd performing the install procedure before you prep and paint the guards. The guards are shipped bare steel, please use caution during the prep and paint process, as the chemicals involved with that operation can be dangerous.

***Vehicle Prep:*** *[The following steps are for both sides]*

**Step 1;** Remove the existing front flare extensions that are on your Jeep YJ models only.

·-c:P,emove any rocker panel molding or any existing OE rocker panels protection.

l,, ·, . .

**Stl1lp , 2:** Th.oroughly clean the entire surface of the body below the door.

*1 ; ): <·*

**Note:** While not required, it may be helpful to loosen the lower three bolts that hold the

* ,flares in place, at the lower end of the front and rear flares.

***Installation:*** *[The following steps are for both sides]*

**Step 1:** Position Jeep on good level surface & set the parking bra ke a nd/or chock tires.

**Step 2:** Loosen all of the body mounts on driver side of the Jeep, there a re 5 per side.

**Step 3:** Raise side of body with floor jack and extension, be sure to jack on or near where the frori,t floor board steps up to the rear floor board. Place your extension inside the frame

,a.ii.., Jacking .outside of the frame will prevent installing your guard.

- :-\C.<· . ·-\: *:;.* ;;-,\_.:\_·1:

**SJEP 4:.** .Position the Rocker Gua rd under the Jeep. Our Rocker Gua rds are designed to sit

011. top 0f the factory body isolators.

**STEP 5:** Position the Rocker Gua rd up tight to the side of the body and raise it to the point that the top of the Gua rd is just below the lowest point of the letters "J E E P" stamped into the side of the Jeep. Once satisfied with the position of the Guard clamp it in place using a "C" clamp or suita ble clamp through the door opening. Use care not to pinch any wires that a re inside the body. Ensure the Rocker guard is level . Use the bottom of the door opening · as a guide.

**STEP 6:** Mark the upper mounting holes on the body using a marker or transfer punch. Remove the Rocker Gua rd and set it aside.

**STEP 7:** Center punch and drill the mounting holes to 3/8"

**STEP 8:** Reinstall the Rocker Gua rd. Install the 3/8" hardware supplied, tighten to 30 ft­ lbs. Lower the Jeep back down on to it's mount and re-install the body mount bolts.

Repeat for opposite side of vehicle.

Drivers side slider Passenger side slider

**Appendix A**

1 8 - 3/8" x I" Stainless Steel Buttonhead bolts 1 8 - 3/8" Top-lock nuts

1 8 - 3/8" washers

***Jeep, CJ, YJ,& TJ are all registered tradenwrk" of the Daimler Cl11J>sler Corp. and are u.,;ed here only as reference points***